# See docs/tracing.txt for syntax documentation.

# hw/intc/apic_common.c
cpu_set_apic_base(uint64_t val) "%016"PRIx64
cpu_get_apic_base(uint64_t val) "%016"PRIx64
# coalescing
apic_report_irq_delivered(int apic_irq_delivered) "coalescing %d"
apic_reset_irq_delivered(int apic_irq_delivered) "old coalescing %d"
apic_get_irq_delivered(int apic_irq_delivered) "returning coalescing %d"

# hw/intc/apic.c
apic_local_deliver(int vector, uint32_t lvt) "vector %d delivery mode %d"
apic_deliver_irq(uint8_t dest, uint8_t dest_mode, uint8_t delivery_mode, uint8_t vector_num, uint8_t trigger_mode) "dest %d dest_mode %d delivery_mode %d vector %d trigger_mode %d"
apic_mem_readl(uint64_t addr, uint32_t val)  "%"PRIx64" = %08x"
apic_mem_writel(uint64_t addr, uint32_t val) "%"PRIx64" = %08x"

# hw/intc/ioapic.c
ioapic_set_remote_irr(int n) "set remote irr for pin %d"
ioapic_clear_remote_irr(int n, int vector) "clear remote irr for pin %d vector %d"
ioapic_eoi_broadcast(int vector) "EOI broadcast for vector %d"
ioapic_mem_read(uint8_t addr, uint8_t size, uint32_t val) "ioapic mem read addr 0x%"PRIx8" size 0x%"PRIx8" retval 0x%"PRIx32
ioapic_mem_write(uint8_t addr, uint8_t size, uint32_t val) "ioapic mem write addr 0x%"PRIx8" size 0x%"PRIx8" val 0x%"PRIx32

# hw/intc/slavio_intctl.c
slavio_intctl_mem_readl(uint32_t cpu, uint64_t addr, uint32_t ret) "read cpu %d reg 0x%"PRIx64" = %x"
slavio_intctl_mem_writel(uint32_t cpu, uint64_t addr, uint32_t val) "write cpu %d reg 0x%"PRIx64" = %x"
slavio_intctl_mem_writel_clear(uint32_t cpu, uint32_t val, uint32_t intreg_pending) "Cleared cpu %d irq mask %x, curmask %x"
slavio_intctl_mem_writel_set(uint32_t cpu, uint32_t val, uint32_t intreg_pending) "Set cpu %d irq mask %x, curmask %x"
slavio_intctlm_mem_readl(uint64_t addr, uint32_t ret) "read system reg 0x%"PRIx64" = %x"
slavio_intctlm_mem_writel(uint64_t addr, uint32_t val) "write system reg 0x%"PRIx64" = %x"
slavio_intctlm_mem_writel_enable(uint32_t val, uint32_t intregm_disabled) "Enabled master irq mask %x, curmask %x"
slavio_intctlm_mem_writel_disable(uint32_t val, uint32_t intregm_disabled) "Disabled master irq mask %x, curmask %x"
slavio_intctlm_mem_writel_target(uint32_t cpu) "Set master irq cpu %d"
slavio_check_interrupts(uint32_t pending, uint32_t intregm_disabled) "pending %x disabled %x"
slavio_set_irq(uint32_t target_cpu, int irq, uint32_t pil, int level) "Set cpu %d irq %d -> pil %d level %d"
slavio_set_timer_irq_cpu(int cpu, int level) "Set cpu %d local timer level %d"

# hw/intc/grlib_irqmp.c
grlib_irqmp_check_irqs(uint32_t pend, uint32_t force, uint32_t mask, uint32_t lvl1, uint32_t lvl2) "pend:0x%04x force:0x%04x mask:0x%04x lvl1:0x%04x lvl0:0x%04x"
grlib_irqmp_ack(int intno) "interrupt:%d"
grlib_irqmp_set_irq(int irq) "Raise CPU IRQ %d"
grlib_irqmp_readl_unknown(uint64_t addr) "addr 0x%"PRIx64
grlib_irqmp_writel_unknown(uint64_t addr, uint32_t value) "addr 0x%"PRIx64" value 0x%x"

# hw/intc/lm32_pic.c
lm32_pic_raise_irq(void) "Raise CPU interrupt"
lm32_pic_lower_irq(void) "Lower CPU interrupt"
lm32_pic_interrupt(int irq, int level) "Set IRQ%d %d"
lm32_pic_set_im(uint32_t im) "im 0x%08x"
lm32_pic_set_ip(uint32_t ip) "ip 0x%08x"
lm32_pic_get_im(uint32_t im) "im 0x%08x"
lm32_pic_get_ip(uint32_t ip) "ip 0x%08x"

# hw/intc/xics.c
xics_icp_check_ipi(int server, uint8_t mfrr) "CPU %d can take IPI mfrr=%#x"
xics_icp_accept(uint32_t old_xirr, uint32_t new_xirr) "icp_accept: XIRR %#"PRIx32"->%#"PRIx32
xics_icp_eoi(int server, uint32_t xirr, uint32_t new_xirr) "icp_eoi: server %d given XIRR %#"PRIx32" new XIRR %#"PRIx32
xics_icp_irq(int server, int nr, uint8_t priority) "cpu %d trying to deliver irq %#"PRIx32" priority %#x"
xics_icp_raise(uint32_t xirr, uint8_t pending_priority) "raising IRQ new XIRR=%#x new pending priority=%#x"
xics_ics_simple_set_irq_msi(int srcno, int nr) "set_irq_msi: srcno %d [irq %#x]"
xics_masked_pending(void) "set_irq_msi: masked pending"
xics_ics_simple_set_irq_lsi(int srcno, int nr) "set_irq_lsi: srcno %d [irq %#x]"
xics_ics_simple_write_xive(int nr, int srcno, int server, uint8_t priority) "ics_write_xive: irq %#x [src %d] server %#x prio %#x"
xics_ics_simple_reject(int nr, int srcno) "reject irq %#x [src %d]"
xics_ics_simple_eoi(int nr) "ics_eoi: irq %#x"
xics_alloc(int irq) "irq %d"
xics_alloc_block(int first, int num, bool lsi, int align) "first irq %d, %d irqs, lsi=%d, alignnum %d"
xics_ics_free(int src, int irq, int num) "Source#%d, first irq %d, %d irqs"
xics_ics_free_warn(int src, int irq) "Source#%d, irq %d is already free"

# hw/intc/s390_flic_kvm.c
flic_create_device(int err) "flic: create device failed %d"
flic_no_device_api(int err) "flic: no Device Contral API support %d"
flic_reset_failed(int err) "flic: reset failed %d"

# hw/intc/s390_flic.c
qemu_s390_airq_suppressed(uint8_t type, uint8_t isc) "flic: adapter I/O interrupt suppressed (type %x isc %x)"
qemu_s390_suppress_airq(uint8_t isc, const char *from, const char *to) "flic: for isc %x, suppress airq by modifying ais mode from %s to %s"

# hw/intc/aspeed_vic.c
aspeed_vic_set_irq(int irq, int level) "Enabling IRQ %d: %d"
aspeed_vic_update_fiq(int flags) "Raising FIQ: %d"
aspeed_vic_update_irq(int flags) "Raising IRQ: %d"
aspeed_vic_read(uint64_t offset, unsigned size, uint32_t value) "From 0x%" PRIx64 " of size %u: 0x%" PRIx32
aspeed_vic_write(uint64_t offset, unsigned size, uint32_t data) "To 0x%" PRIx64 " of size %u: 0x%" PRIx32

# hw/intc/arm_gic.c
gic_enable_irq(int irq) "irq %d enabled"
gic_disable_irq(int irq) "irq %d disabled"
gic_set_irq(int irq, int level, int cpumask, int target) "irq %d level %d cpumask 0x%x target 0x%x"
gic_update_bestirq(int cpu, int irq, int prio, int priority_mask, int running_priority) "cpu %d irq %d priority %d cpu priority mask %d cpu running priority %d"
gic_update_set_irq(int cpu, const char *name, int level) "cpu[%d]: %s = %d"
gic_acknowledge_irq(int cpu, int irq) "cpu %d acknowledged irq %d"

# hw/intc/arm_gicv3_cpuif.c
gicv3_icc_pmr_read(uint32_t cpu, uint64_t val) "GICv3 ICC_PMR read cpu %x value 0x%" PRIx64
gicv3_icc_pmr_write(uint32_t cpu, uint64_t val) "GICv3 ICC_PMR write cpu %x value 0x%" PRIx64
gicv3_icc_bpr_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICC_BPR%d read cpu %x value 0x%" PRIx64
gicv3_icc_bpr_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICC_BPR%d write cpu %x value 0x%" PRIx64
gicv3_icc_ap_read(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICC_AP%dR%d read cpu %x value 0x%" PRIx64
gicv3_icc_ap_write(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICC_AP%dR%d write cpu %x value 0x%" PRIx64
gicv3_icc_igrpen_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICC_IGRPEN%d read cpu %x value 0x%" PRIx64
gicv3_icc_igrpen_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICC_IGRPEN%d write cpu %x value 0x%" PRIx64
gicv3_icc_igrpen1_el3_read(uint32_t cpu, uint64_t val) "GICv3 ICC_IGRPEN1_EL3 read cpu %x value 0x%" PRIx64
gicv3_icc_igrpen1_el3_write(uint32_t cpu, uint64_t val) "GICv3 ICC_IGRPEN1_EL3 write cpu %x value 0x%" PRIx64
gicv3_icc_ctlr_read(uint32_t cpu, uint64_t val) "GICv3 ICC_CTLR read cpu %x value 0x%" PRIx64
gicv3_icc_ctlr_write(uint32_t cpu, uint64_t val) "GICv3 ICC_CTLR write cpu %x value 0x%" PRIx64
gicv3_icc_ctlr_el3_read(uint32_t cpu, uint64_t val) "GICv3 ICC_CTLR_EL3 read cpu %x value 0x%" PRIx64
gicv3_icc_ctlr_el3_write(uint32_t cpu, uint64_t val) "GICv3 ICC_CTLR_EL3 write cpu %x value 0x%" PRIx64
gicv3_cpuif_update(uint32_t cpuid, int irq, int grp, int prio) "GICv3 CPU i/f %x HPPI update: irq %d group %d prio %d"
gicv3_cpuif_set_irqs(uint32_t cpuid, int fiqlevel, int irqlevel) "GICv3 CPU i/f %x HPPI update: setting FIQ %d IRQ %d"
gicv3_icc_generate_sgi(uint32_t cpuid, int irq, int irm, uint32_t aff, uint32_t targetlist) "GICv3 CPU i/f %x generating SGI %d IRM %d target affinity 0x%xxx targetlist 0x%x"
gicv3_icc_iar0_read(uint32_t cpu, uint64_t val) "GICv3 ICC_IAR0 read cpu %x value 0x%" PRIx64
gicv3_icc_iar1_read(uint32_t cpu, uint64_t val) "GICv3 ICC_IAR1 read cpu %x value 0x%" PRIx64
gicv3_icc_eoir_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICC_EOIR%d write cpu %x value 0x%" PRIx64
gicv3_icc_hppir0_read(uint32_t cpu, uint64_t val) "GICv3 ICC_HPPIR0 read cpu %x value 0x%" PRIx64
gicv3_icc_hppir1_read(uint32_t cpu, uint64_t val) "GICv3 ICC_HPPIR1 read cpu %x value 0x%" PRIx64
gicv3_icc_dir_write(uint32_t cpu, uint64_t val) "GICv3 ICC_DIR write cpu %x value 0x%" PRIx64
gicv3_icc_rpr_read(uint32_t cpu, uint64_t val) "GICv3 ICC_RPR read cpu %x value 0x%" PRIx64
gicv3_ich_ap_read(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICH_AP%dR%d read cpu %x value 0x%" PRIx64
gicv3_ich_ap_write(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICH_AP%dR%d write cpu %x value 0x%" PRIx64
gicv3_ich_hcr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_HCR_EL2 read cpu %x value 0x%" PRIx64
gicv3_ich_hcr_write(uint32_t cpu, uint64_t val) "GICv3 ICH_HCR_EL2 write cpu %x value 0x%" PRIx64
gicv3_ich_vmcr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_VMCR_EL2 read cpu %x value 0x%" PRIx64
gicv3_ich_vmcr_write(uint32_t cpu, uint64_t val) "GICv3 ICH_VMCR_EL2 write cpu %x value 0x%" PRIx64
gicv3_ich_lr_read(int regno, uint32_t cpu, uint64_t val) "GICv3 ICH_LR%d_EL2 read cpu %x value 0x%" PRIx64
gicv3_ich_lr32_read(int regno, uint32_t cpu, uint32_t val) "GICv3 ICH_LR%d read cpu %x value 0x%" PRIx32
gicv3_ich_lrc_read(int regno, uint32_t cpu, uint32_t val) "GICv3 ICH_LRC%d read cpu %x value 0x%" PRIx32
gicv3_ich_lr_write(int regno, uint32_t cpu, uint64_t val) "GICv3 ICH_LR%d_EL2 write cpu %x value 0x%" PRIx64
gicv3_ich_lr32_write(int regno, uint32_t cpu, uint32_t val) "GICv3 ICH_LR%d write cpu %x value 0x%" PRIx32
gicv3_ich_lrc_write(int regno, uint32_t cpu, uint32_t val) "GICv3 ICH_LRC%d write cpu %x value 0x%" PRIx32
gicv3_ich_vtr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_VTR read cpu %x value 0x%" PRIx64
gicv3_ich_misr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_MISR read cpu %x value 0x%" PRIx64
gicv3_ich_eisr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_EISR read cpu %x value 0x%" PRIx64
gicv3_ich_elrsr_read(uint32_t cpu, uint64_t val) "GICv3 ICH_ELRSR read cpu %x value 0x%" PRIx64
gicv3_icv_ap_read(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICV_AP%dR%d read cpu %x value 0x%" PRIx64
gicv3_icv_ap_write(int grp, int regno, uint32_t cpu, uint64_t val) "GICv3 ICV_AP%dR%d write cpu %x value 0x%" PRIx64
gicv3_icv_bpr_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_BPR%d read cpu %x value 0x%" PRIx64
gicv3_icv_bpr_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_BPR%d write cpu %x value 0x%" PRIx64
gicv3_icv_pmr_read(uint32_t cpu, uint64_t val) "GICv3 ICV_PMR read cpu %x value 0x%" PRIx64
gicv3_icv_pmr_write(uint32_t cpu, uint64_t val) "GICv3 ICV_PMR write cpu %x value 0x%" PRIx64
gicv3_icv_igrpen_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_IGRPEN%d read cpu %x value 0x%" PRIx64
gicv3_icv_igrpen_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_IGRPEN%d write cpu %x value 0x%" PRIx64
gicv3_icv_ctlr_read(uint32_t cpu, uint64_t val) "GICv3 ICV_CTLR read cpu %x value 0x%" PRIx64
gicv3_icv_ctlr_write(uint32_t cpu, uint64_t val) "GICv3 ICV_CTLR write cpu %x value 0x%" PRIx64
gicv3_icv_rpr_read(uint32_t cpu, uint64_t val) "GICv3 ICV_RPR read cpu %x value 0x%" PRIx64
gicv3_icv_hppir_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_HPPIR%d read cpu %x value 0x%" PRIx64
gicv3_icv_dir_write(uint32_t cpu, uint64_t val) "GICv3 ICV_DIR write cpu %x value 0x%" PRIx64
gicv3_icv_iar_read(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_IAR%d read cpu %x value 0x%" PRIx64
gicv3_icv_eoir_write(int grp, uint32_t cpu, uint64_t val) "GICv3 ICV_EOIR%d write cpu %x value 0x%" PRIx64
gicv3_cpuif_virt_update(uint32_t cpuid, int idx) "GICv3 CPU i/f %x virt HPPI update LR index %d"
gicv3_cpuif_virt_set_irqs(uint32_t cpuid, int fiqlevel, int irqlevel, int maintlevel) "GICv3 CPU i/f %x virt HPPI update: setting FIQ %d IRQ %d maintenance-irq %d"

# hw/intc/arm_gicv3_dist.c
gicv3_dist_read(uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 distributor read: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d"
gicv3_dist_badread(uint64_t offset, unsigned size, bool secure) "GICv3 distributor read: offset 0x%" PRIx64 " size %u secure %d: error"
gicv3_dist_write(uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 distributor write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d"
gicv3_dist_badwrite(uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 distributor write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d: error"
gicv3_dist_set_irq(int irq, int level) "GICv3 distributor interrupt %d level changed to %d"

# hw/intc/arm_gicv3_redist.c
gicv3_redist_read(uint32_t cpu, uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 redistributor %x read: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d"
gicv3_redist_badread(uint32_t cpu, uint64_t offset, unsigned size, bool secure) "GICv3 redistributor %x read: offset 0x%" PRIx64 " size %u secure %d: error"
gicv3_redist_write(uint32_t cpu, uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 redistributor %x write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d"
gicv3_redist_badwrite(uint32_t cpu, uint64_t offset, uint64_t data, unsigned size, bool secure) "GICv3 redistributor %x write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u secure %d: error"
gicv3_redist_set_irq(uint32_t cpu, int irq, int level) "GICv3 redistributor %x interrupt %d level changed to %d"
gicv3_redist_send_sgi(uint32_t cpu, int irq) "GICv3 redistributor %x pending SGI %d"

# hw/intc/armv7m_nvic.c
nvic_recompute_state(int vectpending, int exception_prio) "NVIC state recomputed: vectpending %d exception_prio %d"
nvic_set_prio(int irq, uint8_t prio) "NVIC set irq %d priority %d"
nvic_irq_update(int vectpending, int pendprio, int exception_prio, int level) "NVIC vectpending %d pending prio %d exception_prio %d: setting irq line to %d"
nvic_escalate_prio(int irq, int irqprio, int runprio) "NVIC escalating irq %d to HardFault: insufficient priority %d >= %d"
nvic_escalate_disabled(int irq) "NVIC escalating irq %d to HardFault: disabled"
nvic_set_pending(int irq, int en, int prio) "NVIC set pending irq %d (enabled: %d priority %d)"
nvic_clear_pending(int irq, int en, int prio) "NVIC clear pending irq %d (enabled: %d priority %d)"
nvic_set_pending_level(int irq) "NVIC set pending: irq %d higher prio than vectpending: setting irq line to 1"
nvic_acknowledge_irq(int irq, int prio) "NVIC acknowledge IRQ: %d now active (prio %d)"
nvic_complete_irq(int irq) "NVIC complete IRQ %d"
nvic_set_irq_level(int irq, int level) "NVIC external irq %d level set to %d"
nvic_sysreg_read(uint64_t addr, uint32_t value, unsigned size) "NVIC sysreg read addr 0x%" PRIx64 " data 0x%" PRIx32 " size %u"
nvic_sysreg_write(uint64_t addr, uint32_t value, unsigned size) "NVIC sysreg write addr 0x%" PRIx64 " data 0x%" PRIx32 " size %u"
