# See docs/tracing.txt for syntax documentation.

# hw/sd/milkymist-memcard.c
milkymist_memcard_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_memcard_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
