# Trace events for debugging and performance instrumentation
#
# This file is processed by the tracetool script during the build.
#
# To add a new trace event:
#
# 1. Choose a name for the trace event.  Declare its arguments and format
#    string.
#
# 2. Call the trace event from code using trace_##name, e.g. multiwrite_cb() ->
#    trace_multiwrite_cb().  The source file must #include "trace.h".
#
# Format of a trace event:
#
# [disable] <name>(<type1> <arg1>[, <type2> <arg2>] ...) "<format-string>"
#
# Example: g_malloc(size_t size) "size %zu"
#
# The "disable" keyword will build without the trace event.
#
# The <name> must be a valid as a C function name.
#
# Types should be standard C types.  Use void * for pointers because the trace
# system may not have the necessary headers included.
#
# The <format-string> should be a sprintf()-compatible format string.

# ioport.c
cpu_in(unsigned int addr, char size, unsigned int val) "addr %#x(%c) value %u"
cpu_out(unsigned int addr, char size, unsigned int val) "addr %#x(%c) value %u"

# balloon.c
# Since requests are raised via monitor, not many tracepoints are needed.
balloon_event(void *opaque, unsigned long addr) "opaque %p addr %lu"

# vl.c
vm_state_notify(int running, int reason) "running %d reason %d"
load_file(const char *name, const char *path) "name %s location %s"
runstate_set(int new_state) "new state %d"
system_wakeup_request(int reason) "reason=%d"
qemu_system_shutdown_request(int reason) "reason=%d"
qemu_system_powerdown_request(void) ""

# monitor.c
monitor_protocol_event_handler(uint32_t event, void *qdict) "event=%d data=%p"
monitor_protocol_event_emit(uint32_t event, void *data) "event=%d data=%p"
monitor_protocol_event_queue(uint32_t event, void *qdict, uint64_t rate) "event=%d data=%p rate=%" PRId64
handle_hmp_command(void *mon, const char *cmdline) "mon %p cmdline: %s"
handle_qmp_command(void *mon, const char *req) "mon %p req: %s"

# dma-helpers.c
dma_blk_io(void *dbs, void *bs, int64_t offset, bool to_dev) "dbs=%p bs=%p offset=%" PRId64 " to_dev=%d"
dma_aio_cancel(void *dbs) "dbs=%p"
dma_complete(void *dbs, int ret, void *cb) "dbs=%p ret=%d cb=%p"
dma_blk_cb(void *dbs, int ret) "dbs=%p ret=%d"
dma_map_wait(void *dbs) "dbs=%p"

# memory.c
memory_region_ops_read(int cpu_index, void *mr, uint64_t addr, uint64_t value, unsigned size) "cpu %d mr %p addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_ops_write(int cpu_index, void *mr, uint64_t addr, uint64_t value, unsigned size) "cpu %d mr %p addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_subpage_read(int cpu_index, void *mr, uint64_t offset, uint64_t value, unsigned size) "cpu %d mr %p offset %#"PRIx64" value %#"PRIx64" size %u"
memory_region_subpage_write(int cpu_index, void *mr, uint64_t offset, uint64_t value, unsigned size) "cpu %d mr %p offset %#"PRIx64" value %#"PRIx64" size %u"
memory_region_tb_read(int cpu_index, uint64_t addr, uint64_t value, unsigned size) "cpu %d addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_tb_write(int cpu_index, uint64_t addr, uint64_t value, unsigned size) "cpu %d addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_ram_device_read(int cpu_index, void *mr, uint64_t addr, uint64_t value, unsigned size) "cpu %d mr %p addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_ram_device_write(int cpu_index, void *mr, uint64_t addr, uint64_t value, unsigned size) "cpu %d mr %p addr %#"PRIx64" value %#"PRIx64" size %u"

### Guest events, keep at bottom


## vCPU

# Hot-plug a new virtual (guest) CPU
#
# Mode: user, softmmu
# Targets: all
vcpu guest_cpu_enter(void)

# Hot-unplug a virtual (guest) CPU
#
# Mode: user, softmmu
# Targets: all
vcpu guest_cpu_exit(void)

# Reset the state of a virtual (guest) CPU
#
# Mode: user, softmmu
# Targets: all
vcpu guest_cpu_reset(void)

# @vaddr: Access' virtual address.
# @info : Access' information (see below).
#
# Start virtual memory access (before any potential access violation).
#
# Does not include memory accesses performed by devices.
#
# Access information can be parsed as:
#
# struct mem_info {
#     uint8_t size_shift : 2; /* interpreted as "1 << size_shift" bytes */
#     bool    sign_extend: 1; /* sign-extended */
#     uint8_t endianness : 1; /* 0: little, 1: big */
#     bool    store      : 1; /* wheter it's a store operation */
# };
#
# Mode: user, softmmu
# Targets: TCG(all)
disable vcpu tcg guest_mem_before(TCGv vaddr, uint8_t info) "info=%d", "vaddr=0x%016"PRIx64" info=%d"

# @num: System call number.
# @arg*: System call argument value.
#
# Start executing a guest system call in syscall emulation mode.
#
# Mode: user
# Targets: TCG(all)
disable vcpu guest_user_syscall(uint64_t num, uint64_t arg1, uint64_t arg2, uint64_t arg3, uint64_t arg4, uint64_t arg5, uint64_t arg6, uint64_t arg7, uint64_t arg8) "num=0x%016"PRIx64" arg1=0x%016"PRIx64" arg2=0x%016"PRIx64" arg3=0x%016"PRIx64" arg4=0x%016"PRIx64" arg5=0x%016"PRIx64" arg6=0x%016"PRIx64" arg7=0x%016"PRIx64" arg8=0x%016"PRIx64

# @num: System call number.
# @ret: System call result value.
#
# Finish executing a guest system call in syscall emulation mode.
#
# Mode: user
# Targets: TCG(all)
disable vcpu guest_user_syscall_ret(uint64_t num, uint64_t ret) "num=0x%016"PRIx64" ret=0x%016"PRIx64
