# See docs/tracing.txt for syntax documentation.

# hw/input/ps2.c
ps2_put_keycode(void *opaque, int keycode) "%p keycode %d"
ps2_read_data(void *opaque) "%p"
ps2_set_ledstate(void *s, int ledstate) "%p ledstate %d"
ps2_reset_keyboard(void *s) "%p"
ps2_write_keyboard(void *opaque, int val) "%p val %d"
ps2_keyboard_set_translation(void *opaque, int mode) "%p mode %d"
ps2_mouse_send_packet(void *s, int dx1, int dy1, int dz1, int b) "%p x %d y %d z %d bs %#x"
ps2_mouse_fake_event(void *opaque) "%p"
ps2_write_mouse(void *opaque, int val) "%p val %d"
ps2_kbd_reset(void *opaque) "%p"
ps2_mouse_reset(void *opaque) "%p"
ps2_kbd_init(void *s) "%p"
ps2_mouse_init(void *s) "%p"

# hw/input/milkymist-softusb.c
milkymist_softusb_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_softusb_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_softusb_mevt(uint8_t m) "m %d"
milkymist_softusb_kevt(uint8_t m) "m %d"
milkymist_softusb_pulse_irq(void) "Pulse IRQ"

# hw/input/hid.c
hid_kbd_queue_full(void) "queue full"
hid_kbd_queue_empty(void) "queue empty"

# hw/input/virtio
virtio_input_queue_full(void) "queue full"
